Align Sample

Horizontal

Analog to the other scans, align in the middle of the preview window

Vertical

Top of the Sample Holder to the Bottom of the Camera window (Note Position e.g. as '-7850')

Top of the Sample to the Top of the Camera Window, so you have the full sample inside X Camera Windows (Note Position e.g. as '150')

Stacked scan

Set Name, Angle (-180:180) and Number of Projections in the ControlPanel

Use the Terminal of 'x02da-cons-2' to start the stacked scan with the following command:

/work/sls/bin/stacked_scan.py -t -7850 150 2048 10 1

Parameterlist:

'-t' just tests all Parameters and doesn't run anything. Use this to double-check the positions in the preview

Pos1 (-7850) and Pos2 (150) are the Y-Positions of the Sample at the top and bottom, in MicroMeters

'2048' Number of Lines in Projection (in the camera window). A small overlap is built into the script, so you can use the 'real' number

'10' Magnification

'1' Binning